(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 396)
    (zones 0)
    (modules 49)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (1 Inner1 signal)
    (2 Inner2 signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 130 130)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x310fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Fab/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /CAN1_TX)
  (net 4 /CAN1_RX)
  (net 5 /BOOT0)
  (net 6 /CAN1_EN)
  (net 7 "Net-(C1-Pad1)")
  (net 8 "Net-(R17-Pad1)")
  (net 9 "Net-(R16-Pad1)")
  (net 10 "Net-(C2-Pad2)")
  (net 11 /LEDG)
  (net 12 "Net-(R8-Pad2)")
  (net 13 "Net-(R7-Pad2)")
  (net 14 "Net-(R24-Pad1)")
  (net 15 "Net-(R23-Pad1)")
  (net 16 "Net-(C4-Pad1)")
  (net 17 "Net-(C3-Pad1)")
  (net 18 "Net-(J3-PadD-)")
  (net 19 "Net-(J3-PadD+)")
  (net 20 "Net-(R2-Pad1)")
  (net 21 /DAC1)
  (net 22 "Net-(R1-Pad2)")
  (net 23 /ACCEL1)
  (net 24 /ACCEL2)
  (net 25 "Net-(J3-Pad1)")
  (net 26 "Net-(LED1-PadC)")
  (net 27 "Net-(C15-Pad1)")
  (net 28 /CAN1_L)
  (net 29 /CAN1_H)
  (net 30 /DAC2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ACCEL1)
    (add_net /ACCEL2)
    (add_net /BOOT0)
    (add_net /CAN1_EN)
    (add_net /CAN1_H)
    (add_net /CAN1_L)
    (add_net /CAN1_RX)
    (add_net /CAN1_TX)
    (add_net /DAC1)
    (add_net /DAC2)
    (add_net /LEDG)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-PadD+)")
    (add_net "Net-(J3-PadD-)")
    (add_net "Net-(LED1-PadC)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net VCC)
  )
  (module interceptor:SO08 (layer Top) (tedit 0)
    (at 136.2 96.4 90)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference U6 (at -0.75 0.5 180) (layer F.SilkS))
    (fp_text value MCP6002 (at 0 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 12 "Net-(R8-Pad2)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 13 "Net-(R7-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 21 /DAC1) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 30 /DAC2) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 22 "Net-(R1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module interceptor:HVSON8 (layer Top) (tedit 5F372971)
    (at 145 92.5 90)
    (fp_text reference U3 (at 1.2 1.9 270) (layer F.SilkS))
    (fp_text value TJA1042HVSON (at 0 0 90) (layer F.SilkS) hide)
    (pad PAD smd rect (at 0 0 90) (size 1.6 2.4) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 1.5 0.95 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 1.5 0.35 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 28 /CAN1_L) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 1.5 -0.3 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 29 /CAN1_H) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 1.5 -0.95 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 6 /CAN1_EN) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -1.5 0.95 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 4 /CAN1_RX) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -1.5 0.35 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -1.5 -0.3 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 0.75 0.35) (layers Top F.Paste F.Mask)
      (net 3 /CAN1_TX) (solder_mask_margin 0.1016))
  )
  (module interceptor:USB-A-S (layer Top) (tedit 5F370D33)
    (at 144.311 120.8596 90)
    (descr "<b>USB Series A Surface Mounted</b>")
    (fp_text reference J3 (at -5.3904 -8.311) (layer F.SilkS))
    (fp_text value USB-ASMD-F (at 0 0 90) (layer F.SilkS) hide)
    (pad GND smd rect (at 3.45 3.5 90) (size 3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad D+ smd rect (at 3.45 1 90) (size 3 0.9) (layers Top F.Paste F.Mask)
      (net 19 "Net-(J3-PadD+)") (solder_mask_margin 0.1016))
    (pad VBUS smd rect (at 3.45 -3.5 90) (size 3 0.9) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad D- smd rect (at 3.45 -1 90) (size 3 0.9) (layers Top F.Paste F.Mask)
      (net 18 "Net-(J3-PadD-)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 -6.5659) (size 3.3274 3.3274) (drill 2.3114) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 6.5659) (size 3.3274 3.3274) (drill 2.3114) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 153.0719 99.9152)
    (fp_text reference C1 (at -0.0719 1.8348 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 151.9289 97.2736 90)
    (fp_text reference C10 (at -1.589 -1.162 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 139.2691 111.4616 180)
    (fp_text reference C11 (at -1.589 -1.162) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 153.8847 97.2736 90)
    (fp_text reference C12 (at -0.4764 1.8653 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 136.5767 109.4296 180)
    (fp_text reference C13 (at -1.589 -1.162) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 152.4 92.9 90)
    (fp_text reference C15 (at -1.1 -1.2 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 27 "Net-(C15-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 156.7 92.7 90)
    (fp_text reference C16 (at -1.5 -1.2 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 152.0707 112.5792 180)
    (fp_text reference C2 (at -1.6793 -0.1708) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 135.35 92.2)
    (fp_text reference C26 (at -0.6 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 133.4 101 270)
    (fp_text reference C3 (at -0.5 -1.2 180) (layer F.SilkS))
    (fp_text value 12pF (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 136.2719 106.6356 180)
    (fp_text reference C4 (at -1.589 -1.162) (layer F.SilkS))
    (fp_text value 12pF (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 153.4423 109.328 90)
    (fp_text reference C8 (at -1.589 -1.162 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 135.5 113.25 270)
    (fp_text reference C9 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:RA-RJ45 (layer Top) (tedit 5F370D3A)
    (at 144.25 78.75 180)
    (fp_text reference J15 (at -8.25 -3.65 90) (layer F.SilkS))
    (fp_text value "RJ45 to OBDII" (at 0 0 180) (layer F.SilkS) hide)
    (pad P$2 thru_hole circle (at 7.75 3.05 180) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1 thru_hole circle (at -7.75 3.05 180) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -4.445 -6.35 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 3.175 -6.35 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 0.635 -6.35 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.905 -6.35 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 /CAN1_L) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -3.175 -8.89 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -0.635 -8.89 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.905 -8.89 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 /CAN1_H) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 4.445 -8.89 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at 5.715 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 141 95 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R1 (at -0.635 -0.762 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 22 "Net-(R1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 135.9 116.6)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R13 (at 1.4 0.4 -180) (layer F.SilkS))
    (fp_text value 220 (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 26 "Net-(LED1-PadC)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 11 /LEDG) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 143.7395 114.7636 180)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R16 (at -0.2605 1.5136) (layer F.SilkS))
    (fp_text value 22 (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 18 "Net-(J3-PadD-)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 9 "Net-(R16-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 146.1271 114.7636 180)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R17 (at -2.1229 -0.7364 90) (layer F.SilkS))
    (fp_text value 22 (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 19 "Net-(J3-PadD+)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 8 "Net-(R17-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 131.25 97.5 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R2 (at 2.25 0.75 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 30 /DAC2) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 156.5 103.5)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R23 (at -1 -0.75) (layer F.SilkS))
    (fp_text value 1k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 23 /ACCEL1) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 15 "Net-(R23-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 153.25 114.5)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R24 (at -1.25 1.5 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 24 /ACCEL2) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 14 "Net-(R24-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 150.3 114.9 180)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R25 (at 1.05 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 180) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 14 "Net-(R24-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 154.05 103.5)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R26 (at -1.25 1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 15 "Net-(R23-Pad1)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 141 97.45 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R3 (at -0.635 -0.762 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 21 /DAC1) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 22 "Net-(R1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 131.25 95 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R4 (at -1.2 0.95 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:LQFP64 (layer Top) (tedit 0)
    (at 146.0255 105.518)
    (descr "Based on STM PCB landpattern recomendation")
    (fp_text reference U1 (at -1.56 -0.354) (layer F.SilkS) hide)
    (fp_text value STM32-M-64-LQFP (at -1.814 1.0201) (layer F.Fab) hide)
    (pad 64 smd rect (at -3.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 63 smd rect (at -3.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 62 smd rect (at -2.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 3 /CAN1_TX) (solder_mask_margin 0.1016))
    (pad 61 smd rect (at -2.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 4 /CAN1_RX) (solder_mask_margin 0.1016))
    (pad 60 smd rect (at -1.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 5 /BOOT0) (solder_mask_margin 0.1016))
    (pad 59 smd rect (at -1.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 58 smd rect (at -0.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 57 smd rect (at -0.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 56 smd rect (at 0.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 55 smd rect (at 0.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 6 /CAN1_EN) (solder_mask_margin 0.1016))
    (pad 54 smd rect (at 1.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 53 smd rect (at 1.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 52 smd rect (at 2.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 51 smd rect (at 2.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 50 smd rect (at 3.25 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 49 smd rect (at 3.75 -5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 48 smd rect (at 5.75 -3.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 47 smd rect (at 5.75 -3.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 46 smd rect (at 5.75 -2.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 45 smd rect (at 5.75 -2.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 8 "Net-(R17-Pad1)") (solder_mask_margin 0.1016))
    (pad 44 smd rect (at 5.75 -1.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 9 "Net-(R16-Pad1)") (solder_mask_margin 0.1016))
    (pad 43 smd rect (at 5.75 -1.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 42 smd rect (at 5.75 -0.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 41 smd rect (at 5.75 -0.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 40 smd rect (at 5.75 0.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 39 smd rect (at 5.75 0.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 38 smd rect (at 5.75 1.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 37 smd rect (at 5.75 1.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 36 smd rect (at 5.75 2.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 35 smd rect (at 5.75 2.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 34 smd rect (at 5.75 3.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 33 smd rect (at 5.75 3.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 32 smd rect (at 3.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 31 smd rect (at 3.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
    (pad 30 smd rect (at 2.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 11 /LEDG) (solder_mask_margin 0.1016))
    (pad 29 smd rect (at 2.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 28 smd rect (at 1.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 27 smd rect (at 1.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 26 smd rect (at 0.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 25 smd rect (at 0.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 smd rect (at -0.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 23 smd rect (at -0.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 22 smd rect (at -1.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 21 smd rect (at -1.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 12 "Net-(R8-Pad2)") (solder_mask_margin 0.1016))
    (pad 20 smd rect (at -2.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 13 "Net-(R7-Pad2)") (solder_mask_margin 0.1016))
    (pad 19 smd rect (at -2.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 18 smd rect (at -3.25 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 17 smd rect (at -3.75 5.75) (size 0.3 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 smd rect (at -5.75 3.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 15 smd rect (at -5.75 3.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 14 smd rect (at -5.75 2.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 13 smd rect (at -5.75 2.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at -5.75 1.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 11 smd rect (at -5.75 1.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 smd rect (at -5.75 0.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -5.75 0.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 14 "Net-(R24-Pad1)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -5.75 -0.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 15 "Net-(R23-Pad1)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -5.75 -0.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -5.75 -1.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -5.75 -1.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -5.75 -2.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -5.75 -2.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -5.75 -3.25) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -5.75 -3.75) (size 1.2 0.3) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (module interceptor:SOT23-5 (layer Top) (tedit 0)
    (at 155 88 180)
    (descr "<b>Small Outline Transistor</b>")
    (fp_text reference U2 (at -1.2 3.4 180) (layer F.SilkS))
    (fp_text value MIC52053.3V (at -0.9525 0.1905 180) (layer F.Fab))
    (pad 5 smd rect (at -0.95 -1.3001 180) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 0.95 -1.3001 180) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 27 "Net-(C15-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.95 1.3001 180) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0 1.3001 180) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.95 1.3001 180) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:XTAL-3.2X2.5 (layer Top) (tedit 0)
    (at 137.2117 102.5208 270)
    (fp_text reference Y1 (at 1.9792 2.9117 90) (layer F.SilkS))
    (fp_text value 16MHz (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 1.8 270) (size 1.3 1.1) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 2.3 1.8 270) (size 1.3 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 2.3 0.1 270) (size 1.3 1.1) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 0 0.1 270) (size 1.3 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R locked (layer Top) (tedit 0)
    (at 138 91.75 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R7 (at -0.635 -0.762 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 13 "Net-(R7-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 131.75 91.8)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R8 (at 0.2 1.5) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 12 "Net-(R8-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 148.25 95.75 90)
    (fp_text reference C5 (at -1.589 -1.162 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0603-C (layer Top) (tedit 0)
    (at 141 91.5 270)
    (fp_text reference C6 (at -1.589 -1.162 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 152.7057 117.9386 270)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R5 (at -1.1886 1.4557 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 25 "Net-(J3-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 270) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 5 /BOOT0) (solder_mask_margin 0.1016))
  )
  (module interceptor:0402-R (layer Top) (tedit 0)
    (at 154.0519 117.9386 90)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R6 (at -1.8114 -0.762 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.45 0 90) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 5 /BOOT0) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.45 0 90) (size 0.6 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module interceptor:1X06_NO_SILK_YES_STOP (layer Top) (tedit 0)
    (at 156.8459 118.7006 90)
    (fp_text reference J1 (at -1.2994 -0.5959) (layer F.SilkS))
    (fp_text value M06NO_SILK_YES_STOP (at -1.27 3.175 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /ACCEL1) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /ACCEL2) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module interceptor:1X06_NO_SILK_YES_STOP (layer Top) (tedit 0)
    (at 131.7761 118.7006 90)
    (fp_text reference J2 (at -1.3462 -1.8288) (layer F.SilkS))
    (fp_text value M06NO_SILK_YES_STOP (at -1.27 3.175 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /DAC1) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /DAC2) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer Top) (tedit 5F371A1E)
    (at 132.8 76.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer Top) (tedit 5F371A16)
    (at 155.8 126.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer Top) (tedit 5F371A1B)
    (at 155.8 76.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer Top) (tedit 5F371A12)
    (at 132.8 126.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module interceptor:CHIPLED_0805 (layer Top) (tedit 0)
    (at 134.9 120.75)
    (descr "<b>CHIPLED</b><p>\nSource: http://www.osram.convergy.de/ ... LG_R971.pdf")
    (fp_text reference LED1 (at -1.65 -0.25 -90) (layer F.SilkS))
    (fp_text value LEDCHIPLED_0805 (at 0 0 -90) (layer F.SilkS) hide)
    (pad C smd rect (at 0 -1.05) (size 1.2 1.2) (layers Top F.Paste F.Mask)
      (net 26 "Net-(LED1-PadC)") (solder_mask_margin 0.1016))
    (pad A smd rect (at 0 1.05) (size 1.2 1.2) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module MyFootprints:4pSocket_SMD_Harwin_M22-6540442R (layer Bottom) (tedit 5F38915A)
    (at 139.1 100.4 180)
    (fp_text reference RV1 (at -2.2 11.1 180) (layer B.SilkS))
    (fp_text value Conn_01x04 (at -3.25 13.35 180) (layer B.Fab) hide)
    (pad 4 smd rect (at 3.81 0 180) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.27 0 180) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 2 smd rect (at -1.27 0 180) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 1 smd rect (at -3.81 0 180) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 22 "Net-(R1-Pad2)"))
  )
  (module MyFootprints:4pSocket_SMD_Harwin_M22-6540442R (layer Bottom) (tedit 5F38917C)
    (at 150.6 103.2)
    (fp_text reference RV2 (at -3.5 11.3) (layer B.SilkS))
    (fp_text value Conn_01x04 (at -3.25 13.35) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.81 0) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 30 /DAC2))
    (pad 2 smd rect (at -1.27 0) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 3 smd rect (at 1.27 0) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 4 smd rect (at 3.81 0) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 20 "Net-(R2-Pad1)"))
  )
  (module MyFootprints:4pSocket_SMD_Harwin_M22-6540442R (layer Bottom) (tedit 5F38915F)
    (at 150.5 100.5 180)
    (fp_text reference RV3 (at 3.7 11.2) (layer B.SilkS))
    (fp_text value Conn_01x04 (at -3.25 13.35 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.81 0 180) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 21 /DAC1))
    (pad 2 smd rect (at -1.27 0 180) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 3 smd rect (at 1.27 0 180) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 4 smd rect (at 3.81 0 180) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 22 "Net-(R1-Pad2)"))
  )
  (module MyFootprints:4pSocket_SMD_Harwin_M22-6540442R (layer Bottom) (tedit 5F389176)
    (at 139.1 103.2)
    (fp_text reference RV4 (at 3.8 11.2) (layer B.SilkS))
    (fp_text value Conn_01x04 (at -3.25 13.35) (layer B.Fab) hide)
    (pad 4 smd rect (at 3.81 0) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.27 0) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 2 smd rect (at -1.27 0) (size 1 2) (layers Bottom B.Paste B.Mask))
    (pad 1 smd rect (at -3.81 0) (size 1 2) (layers Bottom B.Paste B.Mask)
      (net 20 "Net-(R2-Pad1)"))
  )
  (module MyFootprints:TestPoint_Loop_D2.50mm_Drill1.0mm (layer Top) (tedit 5F388FFE)
    (at 156.7 99.4)
    (descr "wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference DFU (at 0.9 -2.3 -110) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /BOOT0))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "CH2 HI" (at 153.1 114.4) (layer B.SilkS))
  (gr_text "CH2 LO" (at 138 114.4) (layer B.SilkS))
  (gr_text "CH1 LO" (at 136.2 89.3) (layer B.SilkS))
  (gr_text "CH1 HI" (at 151.1 89.4) (layer B.SilkS))
  (gr_text "PEDAL INTERCEPTOR\nsingle-side version\nj. haupt/j. shuler" (at 130.5 79 270) (layer F.SilkS))
  (gr_line (start 130 130) (end 158.6 130) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.6 130) (end 158.6 72.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.6 72.7) (end 130 72.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130 72.7) (end 130 130) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 133.0461 115.0176 270) (layer F.SilkS))
  (gr_text 2 (at 133.0461 113.3412 270) (layer F.SilkS))
  (gr_text 1 (at 133.0461 105.6704 270) (layer F.SilkS))
  (gr_text OUT (at 130.25 120.25 270) (layer F.SilkS))
  (gr_text IN (at 158 122.25 90) (layer F.SilkS))
  (gr_text 1 (at 155.6521 106.2292 90) (layer F.SilkS))
  (gr_text 2 (at 155.6521 113.9 90) (layer F.SilkS))
  (gr_text GND (at 155.6521 117.0242 90) (layer F.SilkS))
  (gr_text 5V (at 155.6521 119.1832 90) (layer F.SilkS))
  (gr_text GND (at 133.0461 107.6516 270) (layer F.SilkS))
  (gr_text 5V (at 133.0461 110.5726 270) (layer F.SilkS))
  (gr_text 5V (at 133.0461 118.1926 270) (layer F.SilkS))
  (gr_text GND (at 155.6521 109.4042 90) (layer F.SilkS))
  (gr_text 5V (at 155.6521 111.5632 90) (layer F.SilkS))
  (gr_text "PEDAL INTERCEPTOR\nsingle-side version\n j. haupt / j. shuler" (at 157.6 83 90) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2532) (thermal_bridge_width 0.2532))
    (polygon
      (pts
        (xy 141.9361 118.6244) (xy 141.9361 113.7984) (xy 142.8759 112.8586) (xy 143.6379 112.8586) (xy 144.3491 113.5698)
        (xy 144.3745 113.5952) (xy 144.3745 114.1032) (xy 142.8251 114.1032) (xy 142.5965 114.3318) (xy 142.5711 114.3572)
        (xy 142.5711 118.6244)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2532) (thermal_bridge_width 0.2532))
    (polygon
      (pts
        (xy 143.9681 115.932) (xy 144.5777 115.932) (xy 144.5777 118.8022) (xy 143.9681 118.8022)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2532) (thermal_bridge_width 0.2532))
    (polygon
      (pts
        (xy 141.2757 101.4286) (xy 141.2757 100.7936) (xy 141.8599 100.7936) (xy 141.8599 101.4286)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 128.5 71.4) (xy 128.5 131.5) (xy 160 131.5) (xy 160 71.4)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer Inner1) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 129.3 71.9) (xy 129.5 130.5) (xy 159 130.5) (xy 159.3 71.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.5759 115.5764) (xy 155.5759 116.9226) (xy 156.0585 117.4052) (xy 157.8873 117.4052) (xy 158.2429 117.0496)
        (xy 158.2429 115.3224) (xy 157.9127 114.9922) (xy 156.1601 114.9922)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.8937 107.8294) (xy 132.3603 107.296) (xy 130.8109 107.296) (xy 130.3791 107.7278) (xy 130.3791 109.0994)
        (xy 130.3791 109.5312) (xy 130.7347 109.8868) (xy 132.4619 109.8868) (xy 132.8937 109.455)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.0715 115.3986) (xy 132.5381 114.8652) (xy 130.9887 114.8652) (xy 130.5569 115.297) (xy 130.5569 116.6686)
        (xy 130.5569 117.1004) (xy 130.9125 117.456) (xy 132.6397 117.456) (xy 133.0715 117.0242)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.3953 107.7786) (xy 157.8619 107.2452) (xy 156.3125 107.2452) (xy 155.8807 107.677) (xy 155.8807 109.0486)
        (xy 155.8807 109.4804) (xy 156.2363 109.836) (xy 157.9635 109.836) (xy 158.3953 109.4042)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.5635 114.8906) (xy 133.0969 115.424) (xy 133.0969 116.9734) (xy 132.6651 117.4052) (xy 131.2935 117.4052)
        (xy 130.8617 117.4052) (xy 130.5061 117.0496) (xy 130.5061 115.3224) (xy 130.9379 114.8906)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.5127 107.296) (xy 133.0461 107.8294) (xy 133.0461 109.3788) (xy 132.6143 109.8106) (xy 131.2427 109.8106)
        (xy 130.8109 109.8106) (xy 130.4553 109.455) (xy 130.4553 107.7278) (xy 130.8871 107.296)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.6333 107.3722) (xy 158.1667 107.9056) (xy 158.1667 109.455) (xy 157.7349 109.8868) (xy 156.3633 109.8868)
        (xy 155.9315 109.8868) (xy 155.5759 109.5312) (xy 155.5759 107.804) (xy 156.0077 107.3722)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.3285 114.8652) (xy 157.8619 115.3986) (xy 157.8619 116.948) (xy 157.4301 117.3798) (xy 156.0585 117.3798)
        (xy 155.6267 117.3798) (xy 155.2711 117.0242) (xy 155.2711 115.297) (xy 155.7029 114.8652)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 128 71) (xy 161 71) (xy 161 132) (xy 128 132)
      )
    )
  )
)
